**GREENJACKETS BALLPARK**

**NORTH AUGUSTA, SC**

**INTEGRATED ELECTRONIC DISPLAY & SIGNAGE**

GENERAL SCOPE: Provide LED Video Display Product Pricing on ONE (1) Main Display and THREE (3) Ribbon Displays. Pricing includes LED Displays with Lamps, General Mounting Frames with Rear Service for main display and front service for other 3 smaller displays, Engineering Drawings, Operating Software (incl Scoring System, Controllers, & Video Processor) and Operational Training (first 3 home games).

**MAIN LED Video Display (16mm)**

DIMENSIONS: 22’6”H x 42’0”W

MINIMUM RESOLUTION; VIEWING ANGLE: **380x800; 120/120**

MAXIMUM PIXEL PITCH: **16.0mm**

REFRESH RATE/ FRAME RATE: **2880hz; 60fps**

PIXEL CONFIGURATION TYPE: **RGB** lamp

MINIMUM TOTAL NUMBER OF LED PIXELS: **304,000 per face**

DISPLAY QUANTITY: 1 Single Face

SPARE PARTS: 2%

**RIBBON LED Video Displays (16mm)**

DIMENSIONS: 6’-0”H x 80’-0”W

MINIMUM RESOLUTION: **120x1520**

MAXIMUM PIXEL PITCH: **16.0mm**

PIXEL CONFIGURATION TYPE: **RGB** lamp

MINIMUM TOTAL NUMBER OF LED PIXELS: **182,400 per face**

DISPLAY QUANTITY: 3 Single Face

SPARE PARTS: 2%

**Warranty:**

Includes 5 Year Parts & Labor Warranty

Includes 5 Year Parts Warranty (on-site spare parts package)

**Add Options**

1. MENU DISPLAY MONITORS WITH ZONED MEDIA PLAYERS – 22 each @ 52”
2. 2160p 4k Ultra High Definition/ Motion Rate 120
3. 1080p Resolution / Motion Rate 120
4. MENU DISPLAY MONITORS WITH ZONED MEDIA PLAYERS – 22 each @ 50”
5. 2160p 4k Ultra High Definition/ Motion Rate 120
6. 1080p Resolution / Motion Rate 120
7. CONCOURSE OR SUITE DISPLAY MONITORS WITH ZONED MEDIA PLAYERS - 20 each @ 52”
8. 2160p 4k Ultra High Definition/ Motion Rate 120
9. 1080p Resolution / Motion Rate 120
10. CONCOURSE OR SUITE DISPLAY MONITORS WITH ZONED MEDIA PLAYERS - 20 each @ 50”
11. 2160p 4k Ultra High Definition/ Motion Rate 120
12. 1080p Resolution / Motion Rate 120
13. FRONT ENTRY ENTRANCE PYLON – 7’w x 12’h
14. 1st BASE RIBBON LED LINE SCORE BOARD (16MM) 3’ tall x 20’ long